module Base
{
	recipe Repair Ford CVPI Tire
    	{
		fordCVPITire1,
		damnCraft.TireRepairTools,
		damnCraft.TireRepairRubberSolution,
		damnCraft.TireRepairStrips,

		NoBrokenItems:false,
		Result:damnCraft.TireRepairTools,
		Time:250.0,
		OnCreate:DAMN.OnCreate.RepairTire,
		NeedToBeLearn:false,
		CanBeDoneFromFloor:true,
    }

	fixing Fix 92 Ford CVPI Seat
	{
	   Require : 92fordCVPISeatFront1;92fordCVPISeatRear1,
	   ConditionModifier : 0.5,

       Fixer : DuctTape=2;Mechanics=1,
	}
	
	fixing Fix 92 Ford CVPI Trunk Welding
	{
	   Require : 92fordCVPITrunk1,
	   GlobalItem : BlowTorch=5,
	   ConditionModifier : 1.2,

       Fixer : SheetMetal; MetalWelding=3;Mechanics=2,
       Fixer : SmallSheetMetal=2; MetalWelding=3;Mechanics=2,
	}

	fixing Fix 92 Ford CVPI Hood Welding
	{
	   Require : 92fordCVPIEngineDoor1,
	   GlobalItem : BlowTorch=5,
	   ConditionModifier : 1.2,

       Fixer : SheetMetal; MetalWelding=1;Mechanics=2,
       Fixer : SmallSheetMetal=2; MetalWelding=1;Mechanics=2,
	}

   fixing Fix 92 Ford CVPI Hood
	{
	   Require : 92fordCVPIEngineDoor1,
	   GlobalItem : Screws=8,
	   ConditionModifier : 0.5,

       Fixer : SheetMetal; Mechanics=2,
	}

	fixing Fix 92 Ford CVPI Trunk Lid Welding
    {
       Require : 92fordCVPITrunkDoor1,
       GlobalItem : BlowTorch=5,
       ConditionModifier : 1.2,

       Fixer : SheetMetal; MetalWelding=1;Mechanics=2,
       Fixer : SmallSheetMetal=2; MetalWelding=1;Mechanics=2,
    }

   fixing Fix 92 Ford CVPI Trunk Lid
	{
      Require : 92fordCVPITrunkDoor1,
	   GlobalItem : Screws=8,
	   ConditionModifier : 0.5,

       Fixer : SheetMetal; Mechanics=2,
	}

	fixing Fix 92 Ford CVPI Door Welding
	{
	   Require : 92fordCVPIFrontDoor1;92fordCVPIRearDoor1,
	   GlobalItem : BlowTorch=5,
	   ConditionModifier : 1.2,

       Fixer : SheetMetal; MetalWelding=3;Mechanics=3,
       Fixer : SmallSheetMetal=2; MetalWelding=3;Mechanics=3,
	}

	fixing Fix Ford CVPI Armor Welding
    {
       Require : fordCVPIWindshieldArmor;fordCVPIFrontWindowArmor;fordCVPIRearWindowArmor;fordCVPIWindshieldRearArmor,
       GlobalItem : BlowTorch=8,
       ConditionModifier : 1.0,

       Fixer : SheetMetal; MetalWelding=4;Mechanics=4,
       Fixer : SmallSheetMetal=2; MetalWelding=4;Mechanics=4,
    }

	fixing Fix 92 Ford CVPI Armor Welding
    {
       Require : 92fordCVPIBumperFront1;92fordCVPIBumperFront2;92fordCVPIBumperFront3;92fordCVPICabBarrier1,
       GlobalItem : BlowTorch=7,
       ConditionModifier : 1.0,

       Fixer : SheetMetal; MetalWelding=4;Mechanics=4,
       Fixer : SmallSheetMetal=2; MetalWelding=4;Mechanics=4,
    }

    fixing Fix 92 Ford CVPI Plastic Welding
    {
       Require : 92fordCVPIBumperFront0;92fordCVPIBumperRear0,
       GlobalItem : PlasticWeldingGun=250,
       ConditionModifier : 0.85,

       Fixer : PlasticWeldingStaples100Pack; Mechanics=4,
    }

}
